(footprint "gmod-motor-driver"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -0.08 0.68 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "gmod_motor-driver"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer_Name" "PCBCUPID"
		(at -16.002 -37.084 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_circle
		(center -10.16 -8.89)
		(end -10.16 -10.16)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center -10.16 8.89)
		(end -10.16 7.62)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 10.16 -8.89)
		(end 10.16 -10.16)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 10.16 8.89)
		(end 10.16 7.62)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_text user "BIN2"
		(at -3.77444 7.119034 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "STB"
		(at 9.906 -2.64453 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "VM"
		(at -6.775 0.627 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "PWMA"
		(at 6.5278 6.769669 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "MOTOR-DRIVER"
		(at -4.11 -0.16 0)
		(unlocked yes)
		(layer "F.SilkS" knockout)
	)
	(fp_text user "AIN1"
		(at 1.37668 7.115908 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "GND"
		(at -1.27 -7.440641 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "AO-1"
		(at 6.35 -7.366 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "VCC"
		(at 9.906 2.68947 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "BO-2"
		(at -3.81 -7.357794 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "PWMB"
		(at -6.35 6.765761 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "G"
		(at 9.906 0 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "GND"
		(at -6.775 -2.675 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "AIN2"
		(at 3.95224 7.122942 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "GND"
		(at 1.27 -7.440641 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "AO-2"
		(at 3.81 -7.373035 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "BO-1"
		(at -6.35 -7.35076 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "BIN1"
		(at -1.19888 7.112 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 6.35 -10.16 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 3.81 -10.16 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 1.27 -10.16 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -1.27 -10.16 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -3.81 -10.16 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at -6.35 -10.16 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at -8.89 -2.54 270)
		(size 2 2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at -8.89 0 270)
		(size 2 2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at -6.35 10.16 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at -3.81 10.16 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at -1.27 10.16 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 1.27 10.16 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 3.81 10.16 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 6.35 10.16 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 11.43 2.54 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 11.43 0 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 11.43 -2.54 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
)
