(footprint "Glyph-C3"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 21.881617 0.25 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "GLYPH C3"
		(at -0.426743 -1.482983 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at -0.093383 -0.025 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at -0.093383 -0.025 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Name" " "
		(at -31.598402 -12.270935 90)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PARTREV" "v1.0"
		(at 8.45095 -2.38702 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "STANDARD" "Manufacturer Recommendations"
		(at -1.15905 3.17298 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "MAXIMUM_PACKAGE_HEIGHT" "2.55mm"
		(at 5.46095 -1.01702 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "MANUFACTURER" "PCBCUPID"
		(at -0.95905 1.39298 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LINK" "https://shop.pcbcupid.com/product/gd001/"
		(at 0 0 0)
		(layer "Cmts.User")
		(hide yes)
	)
	(attr smd)
	(fp_circle
		(center -22.969038 8.944865)
		(end -24.239038 8.944865)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center -22.86003 -8.848898)
		(end -21.59003 -8.848898)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 22.690224 -8.845135)
		(end 21.420224 -8.845135)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 22.841939 8.894865)
		(end 21.571939 8.894865)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_text user "GLYPH C3"
		(at 23.126617 -3.555 270)
		(unlocked yes)
		(layer "F.SilkS" knockout)
	)
	(fp_text user "SDA"
		(at 16.92 -8.91 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "MI"
		(at 11.89 7.42 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D3"
		(at 6.79 -9.26 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "3V3"
		(at -16.12 6.28 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D-"
		(at 1.63 6.87 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D+"
		(at 4.27 6.88 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "MO"
		(at 9.37 6.92 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "A3"
		(at -0.69 7.15 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D2"
		(at 4.27 -9.23 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "RST"
		(at -5.95 -9.17 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "TX"
		(at 16.95 7.29 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "RST"
		(at -18.61 6.38 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "3V3"
		(at -13.41 6.23 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "A2"
		(at -3.33 7.12 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "SCK"
		(at 6.94 6.22 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "BAT"
		(at -8.43 -9.18 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D1"
		(at 1.64 -9.15 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "A1"
		(at -5.81 7.21 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "RX"
		(at 14.42 7.11 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "USB"
		(at -3.29 -9.29 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D9"
		(at 11.86 -9.09 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "GND"
		(at -10.91 6.09 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "SCL"
		(at 19.23 -8.73 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D0"
		(at -0.82 -9.26 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "GND"
		(at 19.52 6.03 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D8"
		(at 14.36 -9.09 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "NC"
		(at 9.31 -9.09 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "A0"
		(at -8.48 7.22 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at -0.01772 0.967017 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 18.799977 -10.027017 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 16.399977 -10.027017 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 13.799977 -10.027017 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 11.299977 -10.027017 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 8.899977 -10.027017 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 6.199977 -10.127017 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 3.699977 -10.127017 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole oval
		(at 1.099977 -10.127017 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole oval
		(at -1.400023 -10.127017 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole oval
		(at -3.900023 -10.127017 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole oval
		(at -6.500023 -10.127017 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at -9.000023 -10.127017 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at -19.100023 10.172983 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole oval
		(at -16.600023 10.172983 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole oval
		(at -14.000023 10.272983 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole oval
		(at -11.500023 10.272983 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole oval
		(at -9.000023 10.272983 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole oval
		(at -6.400023 10.272983 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole oval
		(at -3.900023 10.272983 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole oval
		(at -1.300023 10.272983 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole oval
		(at 1.199977 10.272983 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole oval
		(at 3.699977 10.272983 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole oval
		(at 6.299977 10.272983 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole oval
		(at 8.799977 10.272983 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole oval
		(at 11.399977 10.272983 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "26" thru_hole oval
		(at 13.899977 10.272983 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "27" thru_hole oval
		(at 16.399977 10.272983 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "28" thru_hole oval
		(at 18.999977 10.172983 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_PCBCUPID_3DMODEL_DIR}/esp32c3.wrl"
		(offset
			(xyz 0 0 4)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
)
