(footprint "gmod-audio-codec"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.27 0.76 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Audio-codec"
		(at 0.186744 -3.502954 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 89.756744 86.767046 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 89.756744 86.767046 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "STANDARD" "Manufacturer Recommendations"
		(at 65.666744 9.107046 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PARTREV" "V1"
		(at 65.666744 9.107046 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "MANUFACTURER" "PCBCUPID"
		(at 65.666744 9.107046 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LINK" "https://shop.pcbcupid.com/product/gm004/"
		(at -0.043256 0.026536 0)
		(layer "Cmts.User")
		(hide yes)
	)
	(attr smd)
	(fp_circle
		(center -10.093256 8.937046)
		(end -8.823256 8.937046)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 10.176744 8.917046)
		(end 11.446744 8.917046)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_text user "CODEC + 3W AMP"
		(at -4.75 -0.09 0)
		(unlocked yes)
		(layer "F.SilkS" knockout)
	)
	(fp_text user "SCL\n"
		(at -0.127 -8.877068 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "LP"
		(at -5.2832 6.5532 270)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "MK"
		(at 2.1082 -8.877068 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "3V3"
		(at -7.9248 -8.840145 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "BCK"
		(at 3.958214 -9.877068 180)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "DAT"
		(at 7.5184 -8.8392 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "GND"
		(at -5.207 -8.877068 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "RN"
		(at 0.6604 6.5024 270)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "LN"
		(at -2.6924 6.5278 270)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "SDA\n"
		(at -2.6162 -8.877068 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "5V"
		(at -10.668 -8.8646 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "RP"
		(at 3.2258 6.477 270)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "LRCK"
		(at 10.668 -8.84045 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 0.256744 -2.132954 180)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 8.837414 -7.536268 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "2" thru_hole oval
		(at 6.297414 -7.536268 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "3" thru_hole oval
		(at 3.757414 -7.536268 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "4" thru_hole oval
		(at 1.217414 -7.536268 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "5" thru_hole oval
		(at -1.322586 -7.536268 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "6" thru_hole oval
		(at -3.862586 -7.536268 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "7" thru_hole oval
		(at -6.402586 -7.536268 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "8" thru_hole oval
		(at -8.942586 -7.536268 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "9" thru_hole oval
		(at -11.482586 -7.536268 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "10" thru_hole circle
		(at -4.675386 7.652932 180)
		(size 2 2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "11" thru_hole circle
		(at -2.135386 7.652932 180)
		(size 2 2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "12" thru_hole circle
		(at 1.273214 7.650532 180)
		(size 2 2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "13" thru_hole circle
		(at 3.813214 7.650532 180)
		(size 2 2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_PCBCUPID_3DMODEL_DIR}/PCBCUPID-AUDIO-CODEC.wrl"
		(offset
			(xyz 0 0 3)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
)
