(footprint "Touch Slider"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.18 -2.39 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Touch Slider"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "MF" "SparkFun Electronics"
		(at 25.4 10 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "MAXIMUM_PACKAGE_HEIGHT" "2.9 mm"
		(at 25.4 10 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Package" "None"
		(at 25.4 10 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Price" "None"
		(at 25.4 10 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Check_prices" "https://www.snapeda.com/parts/PRT-14417/SparkFun+Electronics/view-part/?ref=eda"
		(at 25.4 10 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "STANDARD" "Manufacturer Recommendations"
		(at 25.4 10 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PARTREV" "NA"
		(at 25.4 10 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SnapEDA_Link" "https://www.snapeda.com/parts/PRT-14417/SparkFun+Electronics/view-part/?ref=snap"
		(at 25.4 10 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "MP" "PRT-14417"
		(at 25.4 10 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description_1" "\nQWIIC JST CONNECTOR - SMD 4-PIN\n"
		(at 25.4 10 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Availability" "In Stock"
		(at 25.4 10 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "MANUFACTURER" "SparkFun Electronics"
		(at 25.4 10 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "SCL"
		(at 0.05 -10.01 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "CS3"
		(at 0.22 8.66 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "GND"
		(at -5.18 -9.98 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "TOUCH SLIDER"
		(at 0.06 -0.51 0)
		(unlocked yes)
		(layer "F.SilkS" knockout)
	)
	(fp_text user "3V3"
		(at -7.88 -9.98 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "CS1"
		(at -5.12 8.7 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "INT"
		(at 2.82 -10.03 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "CS2"
		(at -2.57 8.66 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "SDA"
		(at -2.45 -9.94 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(pad "1" thru_hole rect
		(at -6.387751 -8.884839 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at -3.842751 6.355161 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at -3.847751 -8.884839 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at -1.302751 6.355161 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at -1.307751 -8.884839 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 1.237249 6.355161 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 1.232249 -8.884839 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 3.772249 -8.884839 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
)
