(footprint "gsense-magnetometer"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.085858 -0.65 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Magnetometer"
		(at 0.080858 2.15 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at -2.818142 6.484 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at -2.818142 6.484 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_circle
		(center -10.158355 8.871989)
		(end -8.888355 8.871989)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center -10.157957 -8.871593)
		(end -8.887957 -8.871593)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 10.168198 -8.87188)
		(end 11.438198 -8.87188)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 10.187878 8.89148)
		(end 11.457878 8.89148)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_text user "QMC6309\n"
		(at -0.309142 1.11 0)
		(unlocked yes)
		(layer "F.SilkS" knockout)
	)
	(fp_text user "SCL"
		(at 4.4958 -6.4008 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "VCC"
		(at -3.175 -6.3754 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "GND"
		(at -0.508 -6.604 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "SDA"
		(at 1.905 -6.3754 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(pad "1" thru_hole rect
		(at 3.874369 -7.619738 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 1.334369 -7.619738 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at -1.205631 -7.619738 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -3.745631 -7.619738 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_PCBCUPID_3DMODEL_DIR}/PCBCUPID-MAGNETOMETER.wrl"
		(offset
			(xyz 0 0 3.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
)
