(footprint "gmod-relay-1ch"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -0.15 0.62 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "gmod-relay-2ch"
		(at -0.15 1.96 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at -16.85 -0.14 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at -16.85 -0.14 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Exception for pin naming" "The pin one start from left top just because it's confusing for this particular module to start from the right top"
		(at 3.67 -12.96 0)
		(layer "Cmts.User")
		(hide yes)
	)
	(attr smd)
	(fp_text user "IN"
		(at -22.21 4.01 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "COM"
		(at 17.55 1.16 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "NO"
		(at 17.775 6.235 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "VCC"
		(at -23.54 -1.22 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "NC"
		(at 17.65 -3.99 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "RELAY CH1"
		(at 0.06 -0.94 0)
		(unlocked yes)
		(layer "F.SilkS" knockout)
	)
	(fp_text user "GND"
		(at -23.675 1.435 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 0 3.71 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at -19.25 -1.88)
		(size 1.905 1.905)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -19.25 0.72)
		(size 1.905 1.905)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at -19.25 3.22)
		(size 1.905 1.905)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 16.35 5.72)
		(size 1.9 1.9)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 16.35 0.62)
		(size 1.9 1.9)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 16.35 -4.48)
		(size 1.9 1.9)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "D:/KICAD PROJECTS/CH1 relay/PCBCUPID-RELAY-1CH.step"
		(offset (xyz -124.65 87.04 9.5))
		(scale (xyz 1 1 1))
		(rotate (xyz -0 -0 -0))
	)
	(model "C:/Program Files/KiCad/9.0/share/kicad/3dmodels/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
		(offset (xyz -20.65 1.04 -1.5))
		(scale (xyz 1 1 1))
		(rotate (xyz -0 -0 -0))
	)
)
