(footprint "Glyph-H2"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 21.76 -0.22 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "GLYPH H2"
		(at 0.36 -0.26 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0.81 -0.22 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0.81 -0.22 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Name" " "
		(at -30.695019 -12.465935 90)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PARTREV" "v1.0"
		(at 9.354333 -2.58202 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "STANDARD" "Manufacturer Recommendations"
		(at -0.255667 2.97798 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "MAXIMUM_PACKAGE_HEIGHT" "2.55mm"
		(at 6.364333 -1.21202 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "MANUFACTURER" "PCBCUPID"
		(at -0.055667 1.19798 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LINK " "https://shop.pcbcupid.com/product/gd003/"
		(at 0 0 0)
		(layer "Cmts.User")
		(hide yes)
	)
	(attr smd)
	(fp_circle
		(center -22.879015 -8.828118)
		(end -24.149015 -8.828118)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center -22.84591 9.016102)
		(end -21.57591 9.016102)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 22.734584 -8.820135)
		(end 21.464584 -8.820135)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 22.795322 8.969865)
		(end 21.525322 8.969865)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_text user "GLYPH H2"
		(at 22.74 -3.83 270)
		(unlocked yes)
		(layer "F.SilkS" knockout)
	)
	(fp_text user "GND"
		(at 19.6088 6.2738 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "3V3"
		(at -15.875 6.5024 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D-"
		(at 1.8034 7.1628 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D+"
		(at 4.2418 7.14 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D13"
		(at 1.905 -8.9408 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "SCK"
		(at 7.0104 6.4262 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "MO"
		(at 9.5504 7.1882 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "SDA"
		(at 17.1196 -8.8138 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D12"
		(at 4.445 -8.9154 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D0"
		(at -8.2042 7.4676 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "GND"
		(at -10.7696 6.35 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "MI"
		(at 12.065 7.747 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "RST"
		(at -5.715 -8.9154 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "USB"
		(at -3.1496 -8.9408 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "A1"
		(at -5.9436 7.5438 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "RST"
		(at -18.6182 6.604 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "BAT"
		(at -8.2296 -8.8646 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D8"
		(at 11.9888 -8.9662 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "A2"
		(at -3.302 7.5692 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "TX"
		(at 17.0688 7.5692 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D14"
		(at -0.6096 -8.9662 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D9"
		(at 9.6012 -8.89 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "NC"
		(at 14.5034 -8.9154 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "RX"
		(at 14.5288 7.3152 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "SCL"
		(at 19.5326 -8.763 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "3V3"
		(at -13.335 6.62 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "A3"
		(at -0.5334 7.5184 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D10"
		(at 6.8834 -8.9662 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 0.785 1.43 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 18.89 -9.82 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 16.49 -9.82 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 13.89 -9.82 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 11.39 -9.82 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 8.99 -9.82 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 6.29 -9.92 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 3.79 -9.92 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole oval
		(at 1.19 -9.92 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole oval
		(at -1.31 -9.92 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole oval
		(at -3.81 -9.92 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole oval
		(at -6.41 -9.92 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at -8.91 -9.92 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at -19.01 10.38 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole oval
		(at -16.51 10.38 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole oval
		(at -13.91 10.48 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole oval
		(at -11.41 10.48 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole oval
		(at -8.91 10.48 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole oval
		(at -6.31 10.48 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole oval
		(at -3.81 10.48 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole oval
		(at -1.21 10.48 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole oval
		(at 1.29 10.48 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole oval
		(at 3.79 10.48 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole oval
		(at 6.39 10.48 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole oval
		(at 8.89 10.48 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole oval
		(at 11.49 10.48 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "26" thru_hole oval
		(at 13.99 10.48 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "27" thru_hole oval
		(at 16.49 10.48 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "28" thru_hole oval
		(at 19.09 10.38 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_PCBCUPID_3DMODEL_DIR}/esp32h2.wrl"
		(offset
			(xyz 0 0 3.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
)
