(footprint "gmod-flash"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.263001 0.72 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Gmod_FLASH"
		(at -7.16 2.94 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0.133 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0.133 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sim.Pins" "1=K 2=A"
		(at -14.732 -20.187 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "SD3"
		(at 8.74 -2.857 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "MI"
		(at -3.77 -2.797 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "G"
		(at 6.41 -2.887 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "VCC"
		(at -8.89 -2.797 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "CLK"
		(at 3.77 -2.827 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "CS"
		(at -1.27 -2.827 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "MO"
		(at 1.24 -2.797 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "SERIAL-FLASH"
		(at 0 -0.58 0)
		(unlocked yes)
		(layer "F.SilkS" knockout)
	)
	(fp_text user "SD2"
		(at -6.3 -2.797 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at -7.16 4.74 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 8.89 -4.445 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(pad "2" thru_hole circle
		(at 6.35 -4.445 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(pad "3" thru_hole circle
		(at 3.81 -4.445 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(pad "4" thru_hole circle
		(at 1.27 -4.445 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(pad "5" thru_hole circle
		(at -1.27 -4.445 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(pad "6" thru_hole circle
		(at -3.81 -4.445 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(pad "7" thru_hole circle
		(at -6.35 -4.445 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(pad "8" thru_hole circle
		(at -8.89 -4.445 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(embedded_fonts no)
)
