(footprint "gmod-relay-2ch"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.26 0.94 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "gmod-relay-2ch"
		(at 0.05 4.15 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 5.25 -1.9 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 5.25 -1.9 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "MP" "732-10957-ND"
		(at 21.2 24.7 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "RELAY CH2\n"
		(at 0.02 -0.29 0)
		(unlocked yes)
		(layer "F.SilkS" knockout)
	)
	(fp_text user "NO-1"
		(at 22.5044 -6.477 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "IN2"
		(at -17.6276 0.475 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "COM-1"
		(at 23.5458 -2.0574 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "IN1"
		(at -17.7546 -1.9304 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "GND"
		(at -17.0942 2.9464 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "VCC"
		(at -17.272 -4.4196 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "NO-2"
		(at 23.0124 2.9972 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "COM-2"
		(at 23.8506 7.112 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 0.01 2.765 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at -21.536773 -5.132081)
		(size 1.9304 1.9304)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -21.536773 -2.592081)
		(size 1.9304 1.9304)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at -21.536773 -0.052081)
		(size 1.9304 1.9304)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -21.531773 2.462919)
		(size 1.9304 1.9304)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 16.653227 7.527919 270)
		(size 3 3)
		(drill 1.52)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "6" thru_hole circle
		(at 16.653227 2.447919 270)
		(size 3 3)
		(drill 1.52)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "7" thru_hole circle
		(at 16.653227 -2.632081 270)
		(size 3 3)
		(drill 1.52)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "8" thru_hole circle
		(at 16.653227 -7.712081 270)
		(size 3 3)
		(drill 1.52)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(embedded_fonts no)
	(model "D:/KICAD PROJECTS/ch2-RELAY-2CH.step"
		(offset
			(xyz -101 86.5 10.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
	(model "${KICAD9_PCBCUPID_3DMODEL_DIR}/PCBCUPID-RELAY-2CH.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD9_PCBCUPID_3DMODEL_DIR}/gmod-relay-2ch.wrl"
		(offset
			(xyz 0 0 3.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
)
