(footprint "LED_D5.0mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf, generated by kicad-footprint-generator")
	(tags "LED")
	(property "Reference" "REF**"
		(at -0.000001 -3.96 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_D5.0mm"
		(at -0.000001 3.96 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at -1.270001 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at -1.270001 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -0.000001 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at -1.270001 0)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 1.269999 0)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.step"
		(offset
			(xyz -1.270001 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
