(footprint "GLYPH-C6"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 21.6 0.075 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "GLYPH C6"
		(at 0 -0.1 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at -1.485667 -2.47202 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at -1.485667 -2.47202 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Name" " "
		(at -31.505019 -12.445935 90)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PARTREV" "v1.0"
		(at 8.544333 -2.56202 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "STANDARD" "Manufacturer Recommendations"
		(at -1.065667 2.99798 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "MAXIMUM_PACKAGE_HEIGHT" "2.55mm"
		(at 5.554333 -1.19202 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "MANUFACTURER" "PCBCUPID"
		(at -0.865667 1.21798 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LINK" "https://shop.pcbcupid.com/product/gd002/"
		(at 0 0 0)
		(layer "Cmts.User")
		(hide yes)
	)
	(attr through_hole)
	(fp_circle
		(center -22.850985 -8.871882)
		(end -21.580985 -8.871882)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center -22.790247 8.918118)
		(end -21.520247 8.918118)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 22.869015 -8.871882)
		(end 24.139015 -8.871882)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 22.869015 8.908118)
		(end 24.139015 8.908118)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_text user "GLYPH C6"
		(at 22.58 -3.4 270)
		(unlocked yes)
		(layer "F.SilkS" knockout)
	)
	(fp_text user "D20"
		(at 4.3688 6.223 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "3V3"
		(at -15.875 6.223 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "A1"
		(at 9.5 -9 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D7"
		(at 2 -9.15 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "USB"
		(at -3.1496 -9.1948 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D9"
		(at -8.2804 7.112 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "RST"
		(at -5.7658 -9.1948 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D19"
		(at 1.8796 6.1722 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "A0"
		(at 7 -9 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D18"
		(at -0.6858 6.1722 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "RX"
		(at 14.478 7.0866 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "GND"
		(at -10.8712 6.0452 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "RST"
		(at -18.542 6.4516 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "MI"
		(at 12.0142 7.4676 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D15"
		(at -3.2766 6.1468 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "GND"
		(at 19.7104 6.0452 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D8"
		(at -0.635 -9.1694 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D14"
		(at -5.7912 6.1722 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "TX"
		(at 17.1704 7.325 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "A2"
		(at 12 -9 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "SCL"
		(at 19.42 -8.99 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "3V3"
		(at -13.3604 6.277381 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "SCK"
		(at 6.858 6.1468 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "SDA"
		(at 16.93 -9.11 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "A3"
		(at 14.43 -9.11 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D6"
		(at 4.5 -9.15 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "MO"
		(at 9.4742 6.858 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "BAT"
		(at -8.2804 -9.2202 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 0 1.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 18.999753 -10.181882 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 16.459753 -10.181882 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 13.919753 -10.181882 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 11.379753 -10.181882 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 8.839753 -10.181882 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 6.299753 -10.181882 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 3.759753 -10.181882 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole oval
		(at 1.219753 -10.181882 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole oval
		(at -1.320247 -10.181882 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole oval
		(at -3.860247 -10.181882 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole oval
		(at -6.400247 -10.181882 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at -8.940247 -10.181882 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at -19.050247 10.168118 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole oval
		(at -16.510247 10.168118 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole oval
		(at -13.970247 10.168118 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole oval
		(at -11.430247 10.168118 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole oval
		(at -8.890247 10.168118 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole oval
		(at -6.350247 10.168118 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole oval
		(at -3.810247 10.168118 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole oval
		(at -1.270247 10.168118 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole oval
		(at 1.269753 10.168118 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole oval
		(at 3.809753 10.168118 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole oval
		(at 6.349753 10.168118 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole oval
		(at 8.889753 10.168118 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole oval
		(at 11.429753 10.168118 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "26" thru_hole oval
		(at 13.969753 10.168118 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "27" thru_hole oval
		(at 16.509753 10.168118 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "28" thru_hole oval
		(at 19.049753 10.168118 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_PCBCUPID_3DMODEL_DIR}/esp32c6.wrl"
		(offset
			(xyz 0 0 3.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
)
