(footprint "gmod-can"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.16 0.87 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Gmod_CAN"
		(at 1.25 -4.49 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 1.27 0.03 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 1.27 0.03 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LINK" ""
		(at 1.27 0.03 0)
		(layer "Cmts.User")
		(hide yes)
	)
	(attr smd)
	(fp_circle
		(center -10.159999 -8.859999)
		(end -8.889999 -8.859999)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center -10.13 8.91)
		(end -8.86 8.91)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 10.17 -8.89)
		(end 11.44 -8.89)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 10.17 8.91)
		(end 11.44 8.91)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_text user "CAN-TRANSCEIVER"
		(at 0.27 -0.12 0)
		(unlocked yes)
		(layer "F.SilkS" knockout)
	)
	(fp_text user "L"
		(at 1.27 5.364 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "G"
		(at 3.81 5.364 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "H"
		(at -1.27 5.364 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "RX"
		(at 3.66 -7.45 270)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "3V3"
		(at -1.27 -7.21 270)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "TX"
		(at 1.3 -7.735534 270)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "G"
		(at 6.37 -8.21 270)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "5V"
		(at -3.82 -7.77 270)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 1.25 -2.99 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 6.35 -10.13 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 3.81 -10.13 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 1.27 -10.13 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -1.27 -10.13 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -3.81 -10.13 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at -1.275 7.6215)
		(size 2 2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 1.265 7.6215)
		(size 2 2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 3.805 7.6215)
		(size 2 2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_PCBCUPID_3DMODEL_DIR}/gmod_can.wrl"
		(offset
			(xyz 0 0 3)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
)
