(footprint "gmod-rs485"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.225 0.933 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Gmod_RS485"
		(at 0.38 2.25 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0.919568 -0.209195 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0.919568 -0.209195 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sim.Pins" "1=K 2=A"
		(at -12.034432 -28.403195 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_circle
		(center -10.030431 -8.774194)
		(end -8.760431 -8.774194)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center -10.030431 9.005804)
		(end -8.760431 9.005804)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 10.289568 -8.774195)
		(end 11.559568 -8.774195)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 10.289568 9.005805)
		(end 11.559568 9.005805)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_text user "A"
		(at -1.140432 5.195805 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "VCC"
		(at 6.619568 -7.329195 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "G"
		(at -3.690432 -8.119195 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "RS485-TRANSCEIVER"
		(at -0.05 -0.15 0)
		(unlocked yes)
		(layer "F.SilkS" knockout)
	)
	(fp_text user "B"
		(at 1.399568 5.195805 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "TX"
		(at -1.100432 -7.799195 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "G"
		(at 3.939568 5.195805 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "DE"
		(at 1.359568 -7.799195 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "RX"
		(at 3.926868 -7.637039 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 0.48 3.922 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 6.479569 -10.044194 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 3.939569 -10.044194 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 1.399569 -10.044194 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -1.140431 -10.044194 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -3.680431 -10.044194 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at -1.140432 7.735805)
		(size 2 2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 1.399568 7.735805)
		(size 2 2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 3.939568 7.735805)
		(size 2 2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
)
