(footprint "gmod-micro-sd-breakout"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.003641 1.110231 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "MicroSDCard"
		(at -0.016359 5.070231 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0.033641 0.240231 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0.033641 0.240231 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_circle
		(center -10.151063 8.870372)
		(end -8.881063 8.870372)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 10.195141 8.889941)
		(end 11.465141 8.889941)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_text user "MICRO SD CARD\n"
		(at 0.043641 0.110231 0)
		(unlocked yes)
		(layer "F.SilkS" knockout)
	)
	(fp_text user "CS"
		(at 1.9558 -6.6548 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "GND"
		(at 7.0866 -6.6548 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "CD"
		(at 4.5212 -6.604 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "MO"
		(at -3.2004 -6.4516 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "MI"
		(at -0.5842 -6.5786 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D2"
		(at 9.5758 -6.477 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "SCK"
		(at -5.6896 -6.5278 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D1"
		(at -8.255 -6.4516 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "3V3"
		(at -10.7696 -6.4516 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 0.053641 3.460231 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 8.944645 -7.588248 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "2" thru_hole oval
		(at 6.404645 -7.588248 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "3" thru_hole oval
		(at 3.864645 -7.588248 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "4" thru_hole oval
		(at 1.324645 -7.588248 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "5" thru_hole oval
		(at -1.215355 -7.588248 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "6" thru_hole oval
		(at -3.755355 -7.588248 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "7" thru_hole oval
		(at -6.295355 -7.588248 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "8" thru_hole oval
		(at -8.835355 -7.588248 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "9" thru_hole circle
		(at -11.375355 -7.588248 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_PCBCUPID_3DMODEL_DIR}/PCBCUPID-MICRO-SD-CARD.wrl"
		(offset (xyz 0 0 2.5))
		(scale (xyz 1 1 1))
		(rotate (xyz -0 -0 -0))
	)
)
