(footprint "gsense-microphone-1ch"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.241463 0.147521 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "gsense-mic-1ch"
		(at -0.018537 0.847521 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at -1.568537 3.847521 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at -1.568537 3.847521 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "MF" "TDK InvenSense"
		(at 67.511463 11.027521 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_circle
		(center -10.098537 -8.922479)
		(end -8.828537 -8.922479)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center -10.048537 8.917521)
		(end -8.778537 8.917521)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 10.171463 8.897521)
		(end 11.441463 8.897521)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 10.191463 -8.922479)
		(end 11.461463 -8.922479)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_text user "CH1 MIC\n"
		(at 0.281463 -0.722479 0)
		(unlocked yes)
		(layer "F.SilkS" knockout)
	)
	(fp_text user "LR"
		(at 4.6736 -6.8072 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "SCK"
		(at -3.0226 -7.0104 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "VCC"
		(at -5.5118 -7.0104 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "SD"
		(at -0.4318 -6.7818 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "WS"
		(at 2.1336 -6.731 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "GND"
		(at 7.1882 -6.8072 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at -0.088537 1.657521 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -0.088537 1.657521 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -0.088537 1.657521 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -0.088537 1.657521 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 6.590229 -8.084006 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "2" thru_hole circle
		(at 4.050229 -8.084006 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "3" thru_hole circle
		(at 1.510229 -8.084006 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "4" thru_hole circle
		(at -1.029771 -8.084006 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "5" thru_hole circle
		(at -3.569771 -8.084006 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "6" thru_hole circle
		(at -6.109771 -8.084006 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_PCBCUPID_3DMODEL_DIR}/PCB-CUPID-MICROPHONE.wrl"
		(offset
			(xyz 0 0 2)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
)
