(footprint "gsense-microphone-2ch"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.04 1.38 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "MIC-CH2"
		(at 0.04 2.88 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 33.48 2.71 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 33.48 2.71 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "MF" "TDK InvenSense"
		(at 10.155 11.600259 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_circle
		(center -10.095 9.135)
		(end -8.825 9.135)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center -10.07 -8.765)
		(end -8.8 -8.765)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 9.855 9.11)
		(end 11.125 9.11)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 10.205 -8.69)
		(end 11.475 -8.69)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_text user "GND"
		(at 4.54 -2.91 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "SD"
		(at -0.46 -3.93 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "SCK"
		(at -2.76 -2.99 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "WS"
		(at 2.04 -3.73 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "VCC"
		(at -5.64 -3.05 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "MIC CH2\n"
		(at 0 0.57 0)
		(unlocked yes)
		(layer "F.SilkS" knockout)
	)
	(pad "1" thru_hole rect
		(at 3.867382 -7.450479 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "2" thru_hole oval
		(at 1.327382 -7.450479 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "3" thru_hole oval
		(at -1.212618 -7.450479 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "4" thru_hole oval
		(at -3.752618 -7.450479 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "5" thru_hole circle
		(at -6.292618 -7.450479 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(embedded_fonts no)
)
