(footprint "gmod-rtc"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.04 1.03 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "RTC Module"
		(at 0.04 2.53 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0.04 0.3 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0.04 0.3 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "MF" "Harwin"
		(at 25.34 48.8 90)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "MAXIMUM_PACKAGE_HEIGHT" "4.25mm"
		(at 25.34 48.8 90)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "Package" "None"
		(at 25.34 48.8 90)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "Price" "None"
		(at 25.34 48.8 90)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "Check_prices" "https://www.snapeda.com/parts/S8411-45R/Harwin+Inc./view-part/?ref=eda"
		(at 25.34 48.8 90)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "STANDARD" "Manufacturer Recommendations"
		(at 25.34 48.8 90)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "PARTREV" "4"
		(at 25.34 48.8 90)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "SnapEDA_Link" "https://www.snapeda.com/parts/S8411-45R/Harwin+Inc./view-part/?ref=snap"
		(at 25.34 48.8 90)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "MP" "S8411-45R"
		(at 25.34 48.8 90)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "Description_1" "\n                        \n                            Coin Cell Battery Retainer, Horizontal SMT, for CR1220 Coin Cell Batteries, Tape & Reeled\n                        \n"
		(at 25.34 48.8 90)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "Availability" "In Stock"
		(at 25.34 48.8 90)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "MANUFACTURER" "Harwin"
		(at 25.34 48.8 90)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_circle
		(center -10.102083 8.917953)
		(end -8.832083 8.917953)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 10.365 9.125)
		(end 11.635 9.125)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_text user "SCL"
		(at 6.749109 -9.07153 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "VCC\n"
		(at -5.599891 -10.97153 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "CLK"
		(at 1.849109 -8.89653 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "I/B"
		(at -0.690891 -8.89653 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "SDA"
		(at 4.349109 -8.89653 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "GND"
		(at -3.250891 -8.77153 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "RTC MODULE"
		(at 0.06 0.106 0)
		(unlocked yes)
		(layer "F.SilkS" knockout)
	)
	(fp_text user "${REFERENCE}"
		(at 0.04 4.03 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 6.468433 -7.712982 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 3.928433 -7.712982 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 1.388433 -7.712982 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at -1.151567 -7.712982 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at -3.691567 -7.712982 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at -6.231567 -7.712982 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
)
