(footprint "RGB"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "RGB"
		(at 0.439798 -10.266 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_circle
		(center -4.392983 0.234)
		(end -5.154983 -0.02)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 4.243017 0.234)
		(end 5.046236 0.234)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_text user "B"
		(at 1.267017 6.108 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "R"
		(at -3.732983 6.108 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "C"
		(at 3.767017 6.108 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "G"
		(at -1.232983 6.108 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(pad "1" thru_hole rect
		(at -3.352983 7.108 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -0.812983 7.108 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 1.727017 7.108 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 4.267017 7.108 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
)
