(footprint "OLED_128X64_1.3"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.51 -0.74 0)
		(layer "F.SilkS")
	)
	(property "Value" "OLED_128X64_1.3_I2C"
		(at 0.37 1.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "SDA"
		(at 2.661746 -13.34 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "GND"
		(at -4.998254 -13.34 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "SCL"
		(at 0.21 -13.34 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "VCC"
		(at -2.317937 -13.34 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(pad "" np_thru_hole circle
		(at -15.75 -14.85)
		(size 3 3)
		(drill 3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -15.75 14.85)
		(size 3 3)
		(drill 3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 15.75 -14.85)
		(size 3 3)
		(drill 3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 15.75 14.85)
		(size 3 3)
		(drill 3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole circle
		(at 3.81 -15.55)
		(size 1.508 1.508)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "2" thru_hole circle
		(at 1.27 -15.55)
		(size 1.508 1.508)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "3" thru_hole circle
		(at -1.27 -15.55)
		(size 1.508 1.508)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "4" thru_hole rect
		(at -3.81 -15.55)
		(size 1.508 1.508)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(embedded_fonts no)
)
