(footprint "1X6_KEYARRAY"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.246742 -1.282718 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "1X6_KEYARRAY"
		(at 0.246742 -14.282718 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0.246742 -0.782718 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0.246742 -0.782718 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_circle
		(center -22.753258 -8.282718)
		(end -21.483258 -8.282718)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center -22.753258 8.717282)
		(end -21.483258 8.717282)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 22.246742 -8.282718)
		(end 23.516742 -8.282718)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 22.246742 8.717282)
		(end 23.516742 8.717282)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_text user "GND"
		(at -1.163258 -6.622718 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "VCC"
		(at -4.163258 -6.622718 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "KEY"
		(at 2.336742 -6.622718 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(pad "1" thru_hole rect
		(at 2.746742 -9.282718 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(pad "2" thru_hole circle
		(at 0.206742 -9.282718 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(pad "3" thru_hole circle
		(at -2.333258 -9.282718 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(embedded_fonts no)
)
