(footprint "usb-c"(version 20241229) (generator "pcbnew") (generator_version "9.0")(layer "F.Cu" )(property "Reference" "REF**"(at 0 -0.5 0)(unlocked yes)(layer "F.SilkS" )(hide yes))(property "Value" "usb-c"(at -0.4 0.71 180)(unlocked yes)(layer "F.Fab" ))(property "Datasheet" ""(at 0 0 0)(unlocked yes)(layer "F.Fab" )(hide yes))(property "Description" ""(at 0 0 0)(unlocked yes)(layer "F.Fab" )(hide yes))(attr smd)(fp_text user "D+"(at 1.9558 -7.0612 90)(unlocked yes)(layer "B.SilkS" ))(fp_text user "GND"(at 7.2898 -7.3152 90)(unlocked yes)(layer "B.SilkS" ))(fp_text user "D-"(at -0.508 -7.0612 90)(unlocked yes)(layer "B.SilkS" ))(fp_text user "CC2"(at 4.5212 -7.2644 90)(unlocked yes)(layer "B.SilkS" ))(fp_text user "CC1"(at -2.9464 -7.239 90)(unlocked yes)(layer "B.SilkS" ))(fp_text user "VBUS"(at -5.5372 -7.3152 90)(unlocked yes)(layer "B.SilkS" ))(pad "1" thru_hole circle(at 6.454 -9.91 270)(size 1.7 1.7)(drill 1)(layers  "*.Cu" "*.Mask")(remove_unused_layers no))(pad "2" thru_hole circle(at 3.914 -9.91 270)(size 1.7 1.7)(drill 1)(layers  "*.Cu" "*.Mask")(remove_unused_layers no))(pad "3" thru_hole circle(at 1.374 -9.91 270)(size 1.7 1.7)(drill 1)(layers  "*.Cu" "*.Mask")(remove_unused_layers no))(pad "4" thru_hole circle(at -1.166 -9.91 270)(size 1.7 1.7)(drill 1)(layers  "*.Cu" "*.Mask")(remove_unused_layers no))(pad "5" thru_hole circle(at -3.706 -9.91 270)(size 1.7 1.7)(drill 1)(layers  "*.Cu" "*.Mask")(remove_unused_layers no))(pad "6" thru_hole rect(at -6.246 -9.91 270)(size 1.7 1.7)(drill 1)(layers  "*.Cu" "*.Mask")(remove_unused_layers no))(embedded_fonts no))