(footprint "1X3_KEYARRAY"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "1X3_KEYARRAY"
		(at -0.5 -14 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_line
		(start -26.37947 8.427472)
		(end -26.379211 -9.319776)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -23.821192 -11.859869)
		(end 21.916983 -11.859868)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 21.839361 11.00013)
		(end -23.83936 10.99987)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 24.456523 -9.275792)
		(end 24.420166 8.470652)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -26.379211 -9.319776)
		(mid -25.618505 -11.122103)
		(end -23.821192 -11.859869)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -23.83936 10.99987)
		(mid -25.641777 10.239101)
		(end -26.37947 8.427472)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 21.916983 -11.859868)
		(mid 23.722983 -11.095022)
		(end 24.456523 -9.275792)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 24.420166 8.470652)
		(mid 23.650773 10.271022)
		(end 21.839361 11.00013)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center -24 -8.77)
		(end -22.73 -8.77)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center -24 8)
		(end -22.73 8)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 22 -9)
		(end 23.27 -9)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 22 8)
		(end 23.27 8)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_text user "D2"
		(at 1.5 -7 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "D1"
		(at -0.5 -7 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "VCC"
		(at -7 -7 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "GND"
		(at -4 -7 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "D3"
		(at 4 -7 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(pad "1" thru_hole rect
		(at -5.16 -9.5 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(pad "2" thru_hole circle
		(at -2.62 -9.5 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(pad "3" thru_hole circle
		(at -0.08 -9.5 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(pad "4" thru_hole circle
		(at 2.46 -9.5 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(pad "5" thru_hole circle
		(at 5 -9.5 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(embedded_fonts no)
)
