(footprint "limit switch"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "limit switch"
		(at 0 11.8 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_circle
		(center -7.8 -7.744889)
		(end -6.055111 -7.744889)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center -7.8 7.855111)
		(end -6.055111 7.855111)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 7.8 -7.744889)
		(end 9.544889 -7.744889)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 7.8 7.855111)
		(end 9.544889 7.855111)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_text user "S"
		(at -2.2 6.4 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "V"
		(at 3.2 6.2 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "NC"
		(at 7 -2.2 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "C"
		(at -5 -2 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "G"
		(at 0.6 6.4 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "NO"
		(at 1 -2.2 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(pad "1" thru_hole circle
		(at 2.6 3.8)
		(size 1.508 1.508)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "2" thru_hole circle
		(at 0 3.8)
		(size 1.508 1.508)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "3" thru_hole circle
		(at -2.8 3.8)
		(size 1.508 1.508)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "4" thru_hole circle
		(at -5.6 -0.8)
		(size 1.508 1.508)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "5" thru_hole circle
		(at 0 -0.8)
		(size 1.508 1.508)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "6" thru_hole circle
		(at 6 -0.8)
		(size 1.508 1.508)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(embedded_fonts no)
)
