(footprint "RGB_THT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 16.6 -0.2 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "RGB_THT"
		(at -0.2 5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "C"
		(at 3.8 2.8 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "B"
		(at 1.8 2.8 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "R"
		(at -2.6 2.8 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "G"
		(at -0.4 2.8 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 16.8 -2.6 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at -3.2385 0.200001)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -1.0795 0.200001)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 1.0795 0.200001)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 3.2385 0.200001)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
)
