(footprint "LCD_DISPLAY"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "LCD_DISPLAY"
		(at 0.31 -25.94 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_circle
		(center -57.52843 18.54)
		(end -55.79 18.69)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center -57.5 -18.54)
		(end -55.755111 -18.54)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 57.5 -18.474889)
		(end 59.23843 -18.324889)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 57.51 18.515111)
		(end 59.24843 18.665111)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_text user "RW"
		(at 27.99 -23.97 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "DB3"
		(at 40.47 -23.81 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "DB5"
		(at 45.73 -23.81 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "DB1"
		(at 35.48 -23.86 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "V0/VEE"
		(at 22.79 -23.81 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "K(LED-)"
		(at 15.25 -23.97 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "VDD"
		(at 20.4 -24.02 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "DB2"
		(at 38.03 -23.86 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "DB0"
		(at 32.93 -23.92 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "A(LED+)"
		(at 12.43 -24.02 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "RS"
		(at 25.5 -23.86 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "VSS"
		(at 18 -23.86 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "E"
		(at 30.38 -23.81 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "DB7"
		(at 50.83 -23.81 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "DB4"
		(at 43.23 -23.92 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "DB6"
		(at 48.33 -23.86 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(pad "1" thru_hole rect
		(at 17 -19.46 180)
		(size 1.5 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 19.54 -19.46 180)
		(size 1.5 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 22.08 -19.46 180)
		(size 1.5 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 24.62 -19.46 180)
		(size 1.5 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 27.16 -19.46 180)
		(size 1.5 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 29.7 -19.46 180)
		(size 1.5 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 32.24 -19.46 180)
		(size 1.5 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole oval
		(at 34.78 -19.46 180)
		(size 1.5 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole oval
		(at 37.32 -19.46 180)
		(size 1.5 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole oval
		(at 39.86 -19.46 180)
		(size 1.5 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole oval
		(at 42.4 -19.46 180)
		(size 1.5 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole oval
		(at 44.94 -19.46 180)
		(size 1.5 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole oval
		(at 47.48 -19.46 180)
		(size 1.5 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole oval
		(at 50.02 -19.46 180)
		(size 1.5 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole oval
		(at 14.46 -19.46 180)
		(size 1.5 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole oval
		(at 11.92 -19.46 180)
		(size 1.5 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
)
