(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "LCD-16X2"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 23.368 0)
		)
		(property "Value" "LCD-16X2"
			(at -7.62 -22.86 0)
		)
		(property "Footprint" ""
			(at 40.005 -6.985 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "MF" ""
			(at 20.32 -12.065 0)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 24.13 8.255 0)
		)
		(property "Package" ""
			(at 28.575 -2.54 0)
		)
		(property "Price" ""
			(at 31.115 -12.7 0)
		)
		(property "Check_prices" ""
			(at -62.865 -8.89 0)
		)
		(property "STANDARD" ""
			(at 29.21 1.905 0)
		)
		(property "PARTREV" ""
			(at 20.32 -2.54 0)
		)
		(property "SnapEDA_Link" ""
			(at -62.865 -13.97 0)
		)
		(property "MP" "LCD-16X2"
			(at 1.27 -16.51 0)
		)
		(property "Description_1" ""
			(at -57.785 -19.685 0)
		)
		(property "Availability" ""
			(at 41.91 -12.7 0)
		)
		(property "MANUFACTURER" ""
			(at 34.29 -8.89 0)
		)
		(symbol "LCD-16X2_0_0"
			(text "16x2 LCD"
				(at 5.08 -6.858 900)
			)
			(pin power_in line
				(at -12.7 20.32 0)
				(length 5.08)
				(name "VSS")
				(number "1")
			)
			(pin power_in line
				(at -12.7 17.78 0)
				(length 5.08)
				(name "VDD")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "VO")
				(number "3")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "RS")
				(number "4")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "R/W")
				(number "5")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "E")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "DB0")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "DB1")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 5.08)
				(name "DB2")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "DB3")
				(number "10")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "DB4")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "DB5")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "DB6")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "DB7")
				(number "14")
			)
			(pin power_in line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "A")
				(number "15")
			)
			(pin power_in line
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "K")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
)
