(footprint "CherryMX"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Cherry MX switch footprint. Size: 10.00u, Mount type: Plate, Using Kailh Socket: yes, Stabilizer: Plate mounted, Lighting: 2 pin LED")
	(tags "CherryMX 10.00u KailhSocket LED")
	(property "Reference" "REF**"
		(at 0 -8.6625 0)
		(layer "F.SilkS")
	)
	(property "Value" "CherryMX"
		(at 0 8.6625 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "LED_K"
		(at 1.64 10.12 0)
		(unlocked yes)
		(layer "User.4")
	)
	(fp_text user "LED_A"
		(at -4.84 9.98 0)
		(unlocked yes)
		(layer "User.4")
	)
	(fp_text user "PIN 1"
		(at -16.38 -1.64 0)
		(unlocked yes)
		(layer "User.4")
	)
	(fp_text user "PIN 2"
		(at 8.79 -4.64 0)
		(unlocked yes)
		(layer "User.4")
	)
	(pad "" np_thru_hole circle
		(at -3.81 -2.54)
		(size 3 3)
		(drill 3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0 0)
		(size 4 4)
		(drill 4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.54 -5.08)
		(size 3 3)
		(drill 3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -7.41 -2.54)
		(size 2.55 2.5)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "2" smd rect
		(at 6.015 -5.08)
		(size 2.55 2.5)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "3" thru_hole circle
		(at -1.27 5.08)
		(size 1.6906 1.6906)
		(drill 0.9906)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 1.27 5.08)
		(size 1.6906 1.6906)
		(drill 0.9906)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/models/KailhSocket.stp"
		(offset
			(xyz -0.6 3.8 -3.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 180)
		)
	)
)
