(footprint "OLED 0.91 DISPLAY"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -17.1 1.505 90)
		(layer "F.SilkS")
	)
	(property "Value" "OLED 0.91 DISPLAY"
		(at 18.5 14 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "VCC"
		(at 15.5 3.26 270)
		(layer "F.SilkS")
	)
	(fp_text user "SDA"
		(at 15.38 -2.09 270)
		(layer "F.SilkS")
	)
	(fp_text user "SCL"
		(at 15.5 0.6 270)
		(layer "F.SilkS")
	)
	(fp_text user "GND"
		(at 15.53 5.83 270)
		(layer "F.SilkS")
	)
	(fp_text user "OLED Panel"
		(at 0 1.595 0)
		(layer "F.SilkS")
	)
	(pad "1" thru_hole rect
		(at 17.5 -2.215)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 17.5 0.325)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 17.5 2.865)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 17.5 5.405)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
)
