(footprint "ultrasonic_sensor"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 6.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "ultrasonic_sensor"
		(at 0.25 3.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "GND"
		(at -3.2 13.8 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "TRIG"
		(at 1.8 13.6 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "VCC"
		(at 4.4 14 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "ECHO"
		(at -0.8 12.8 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 0.25 1.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 4 18.4)
		(size 1.53 1.53)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "2" thru_hole circle
		(at 1.4 18.4)
		(size 1.53 1.53)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "3" thru_hole circle
		(at -1.2 18.4)
		(size 1.53 1.53)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "4" thru_hole circle
		(at -3.6 18.4)
		(size 1.53 1.53)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(embedded_fonts no)
)
