(footprint "D_DO-41_SOD81_P10.16mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, length*diameter=5.2*2.7mm^2, https://www.diodes.com/assets/Package-Files/DO-41-Plastic.pdf")
	(tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
	(property "Reference" "D1"
		(at 5.08 0 0)
		(layer "F.SilkS")
	)
	(property "Value" "1N4001"
		(at 5.08 2.47 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" "50V 1A General Purpose Rectifier Diode, DO-41"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sim.Device" "D"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sim.Pins" "1=K 2=A"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.2 2.2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.113636)
	)
	(pad "2" thru_hole circle
		(at 10.16 0)
		(size 2.2 2.2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.step"
		(offset (xyz 0 0 0))
		(scale (xyz 1 1 1))
		(rotate (xyz 0 0 0))
	)
)
