(footprint "POTENTIOMETER 90'"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "POTENTIOMETER 90'"
		(at 3.1655 -8.35 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "CW"
		(at 6.2755 2.94 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "CCW"
		(at 5.6755 -1.98 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "OUTPUT"
		(at 4.7655 0.31 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(pad "1" thru_hole rect
		(at 8.9555 -2.54 180)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 8.9555 -0.04 180)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 8.9555 2.46 180)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
)
