(footprint "JST_EH_S4B-EH_1x04_P2.50mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "JST EH series connector, S4B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
	(tags "connector JST EH horizontal")
	(property "Reference" "REF**"
		(at 0 -5.44 0)
		(layer "F.SilkS")
	)
	(property "Value" "JST_EH_S4B-EH_1x04_P2.50mm_Horizontal"
		(at 0 5.16 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at -3.75 2.46 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at -3.75 2.46 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 3.75 -2.6 180)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.147059)
	)
	(pad "2" thru_hole oval
		(at 1.25 -2.6 180)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at -1.25 -2.6 180)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at -3.75 -2.6 180)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_EH_S4B-EH_1x04_P2.50mm_Horizontal.step"
		(offset
			(xyz -3.75 -2.46 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
