(footprint "BC547(NPN)"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
	(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
	(property "Reference" "REF**"
		(at 1.27 -3.56 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "BC547(NPN)"
		(at -7.6 0 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "BASE"
		(at 4.225 0.625 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "EMITTER"
		(at -3.6 5.4 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "COLLECTOR"
		(at -3.6 -4.2 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(pad "1" thru_hole rect
		(at -0.375 -1.645 270)
		(size 1.05 1.5)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at -0.375 -0.375 270)
		(size 1.05 1.5)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at -0.375 0.895 270)
		(size 1.05 1.5)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.step"
		(offset (xyz 0 0 0))
		(scale (xyz 1 1 1))
		(rotate (xyz 0 0 0))
	)
)
