(footprint "GLYPH RP 2040 MINI"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -17.675 -2.415 90)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Value" "GLYPH MINI 2040"
		(at -15.675 -1.915 90)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer_Name" ""
		(at 31 17.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer_Part_Number" ""
		(at 31 17.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LCSC_Part" ""
		(at 31 17.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer_Name_2" ""
		(at 31 17.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer_Part_Number_2" ""
		(at 31 17.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "0"
		(at -10.085 -6.675 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "13"
		(at 8.825 5.585 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "27"
		(at 1.825 6.585 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "9"
		(at 8.825 -4.415 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "12"
		(at 8.825 3.085 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "GND"
		(at -8.175 6.585 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "28"
		(at -0.675 6.585 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "6"
		(at 4.325 -6.915 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "11"
		(at 8.825 0.585 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "2"
		(at -5.675 -6.915 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "1"
		(at -7.915 -6.825 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "15"
		(at 6.825 6.585 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "5"
		(at 1.825 -6.915 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "26"
		(at 4.825 6.585 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "3"
		(at -3.175 -6.915 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "7"
		(at 6.915 -6.915 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "10"
		(at 8.825 -1.915 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "4"
		(at -0.675 -6.915 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "14"
		(at 9.325 7.585 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "8"
		(at 9.825 -5.915 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "29"
		(at -3.175 6.585 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "3V3"
		(at -5.675 6.585 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "5V"
		(at -10.175 6.085 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(pad "1" thru_hole rect
		(at 10.25 -9.25 90)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole oval
		(at 10.25 -7.75 90)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole rect
		(at 7.71 -9.25 90)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 7.71 -7.75 90)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole rect
		(at 5.17 -9.25 90)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 5.17 -7.75 90)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole rect
		(at 2.63 -9.25 90)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 2.63 -7.75 90)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole rect
		(at 0.09 -9.25 90)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 0.09 -7.75 90)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole rect
		(at -2.45 -9.25 90)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at -2.45 -7.75 90)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole rect
		(at -4.99 -9.25 90)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at -4.99 -7.75 90)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole rect
		(at -7.53 -9.25 90)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole oval
		(at -7.53 -7.75 90)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole rect
		(at -10.07 -9.25 90)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole rect
		(at -10.07 -7.75 90)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole oval
		(at -10.040229 7.508988 270)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole rect
		(at -10.040229 9.008988 270)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole oval
		(at -7.500229 7.508988 270)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole rect
		(at -7.500229 9.008988 270)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole oval
		(at -4.960229 7.508988 270)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole rect
		(at -4.960229 9.008988 270)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole oval
		(at -2.420229 7.508988 270)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole rect
		(at -2.420229 9.008988 270)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole oval
		(at 0.119771 7.508988 270)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole rect
		(at 0.119771 9.008988 270)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole oval
		(at 2.659771 7.508988 270)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole rect
		(at 2.659771 9.008988 270)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole oval
		(at 5.199771 7.508988 270)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole rect
		(at 5.199771 9.008988 270)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole oval
		(at 7.739771 7.508988 270)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole rect
		(at 7.739771 9.008988 270)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole rect
		(at 10.279771 9.008988 270)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole oval
		(at 10.245157 4.960996)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole rect
		(at 11.745157 4.960996)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole oval
		(at 10.245157 2.420996)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole rect
		(at 11.745157 2.420996)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole oval
		(at 10.245157 -0.119004)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole rect
		(at 11.745157 -0.119004)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole oval
		(at 10.245157 -2.659004)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole rect
		(at 11.745157 -2.659004)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole rect
		(at 10.245157 -5.199004)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole rect
		(at 11.745157 -5.199004)
		(size 2 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "118" thru_hole rect
		(at 10.279771 7.508988 270)
		(size 2.5 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
)
