(footprint "rotaryencoder"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "rotaryencoder"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "GND"
		(at -1.8 11.2 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "DT"
		(at 3 -7.8 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "MOUNTING"
		(at -15.6 0.6 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "MOUNTING"
		(at 9.63 0.73 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "CLK"
		(at -1.6 -7.6 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "VCC"
		(at 0.6 11 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "SWITCH"
		(at 3.2 13.6 90)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(pad "1" thru_hole rect
		(at -2.4 -5.8)
		(size 1.65 1.65)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "2" thru_hole circle
		(at 2.4 -5.8)
		(size 1.65 1.65)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "3" thru_hole circle
		(at 2.4 5.8)
		(size 1.65 1.65)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "4" thru_hole circle
		(at 0 5.835)
		(size 1.65 1.65)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "5" thru_hole circle
		(at -2.6 5.8)
		(size 1.65 1.65)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "S1" thru_hole oval
		(at -6 -0.2)
		(size 3 6)
		(drill oval 2 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "S2" thru_hole oval
		(at 6 -0.2)
		(size 3 6)
		(drill oval 2 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(embedded_fonts no)
)
