(footprint "JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "JST XH series connector, B4B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
	(tags "connector JST XH vertical")
	(property "Reference" "REF**"
		(at 0.002788 -4.076319 0)
		(layer "F.SilkS")
	)
	(property "Value" "JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical"
		(at 0.002788 4.073681 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at -3.747212 -0.526319 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at -3.747212 -0.526319 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0.002788 2.173681 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at -3.747212 -0.526319)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.147059)
	)
	(pad "2" thru_hole oval
		(at -1.247212 -0.526319)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 1.252788 -0.526319)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 3.752788 -0.526319)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical.step"
		(offset
			(xyz -3.747212 0.526319 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
