(footprint "BC557_pnp"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "<b>SOT-54</b><p>grid 2.54 mm")
	(property "Reference" "REF**"
		(at 6.3594 -0.63594 0)
		(layer "F.SilkS")
	)
	(property "Value" "BC557_pnp"
		(at 6.99853 1.27246 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0.04 3.48 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "B" thru_hole circle
		(at 0 -1.905)
		(size 1.3208 1.3208)
		(drill 0.8128)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "C" thru_hole circle
		(at -1.27 0)
		(size 1.3208 1.3208)
		(drill 0.8128)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "E" thru_hole circle
		(at 1.27 0)
		(size 1.3208 1.3208)
		(drill 0.8128)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(embedded_fonts no)
	(model "${KICAD9_PCBCUPID_3DMODEL_DIR}/BC557.STEP"
		(offset (xyz 0 0 0))
		(scale (xyz 1 1 1))
		(rotate (xyz -0 -0 -0))
	)
)
