(footprint "DHT_11"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -4.775 -13.595 0)
		(layer "F.SilkS")
	)
	(property "Value" "DHT_11"
		(at 0 21.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "NC"
		(at 9 2.2 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "GND"
		(at 8.8 4.6 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "VDD"
		(at 8.8 -3 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "DT"
		(at 8.8 -0.8 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(pad "1" thru_hole rect
		(at 0 -3.82)
		(size 1.5 1.5)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 -1.28)
		(size 1.5 1.5)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 1.26)
		(size 1.5 1.5)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 3.8)
		(size 1.5 1.5)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
)
