(footprint "hall_sensor"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.376 -3.715 0)
		(layer "F.SilkS")
	)
	(property "Value" "hall_sensor"
		(at -0.06 3.88 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -0.037539 5.63 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -0.037539 5.63 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -0.037539 5.63 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -0.037539 5.63 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole oval
		(at -1.27 0)
		(size 1.1 2.2)
		(drill 0.79)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "2" thru_hole oval
		(at 0 0)
		(size 1.1 2.2)
		(drill 0.79)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "3" thru_hole oval
		(at 1.27 0)
		(size 1.1 2.2)
		(drill 0.79)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(embedded_fonts no)
	(model "${KICAD9_PCBCUPID_3DMODEL_DIR}/hall_sensor.STEP"
		(offset (xyz 0 0 -1.5))
		(scale (xyz 1 1 1))
		(rotate (xyz -90 -0 -180))
	)
)
