(footprint "PUSH TO LOCK BUTTON"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DPDT Latching")
	(tags "SW DPDT")
	(property "Reference" "REF**"
		(at 0.635 -9.525 180)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "PUSH TO LOCK BUTTON"
		(at 0.6 14.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "COM2"
		(at 0.6 1.2 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "NO1"
		(at 3.2 -0.8 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "COM1"
		(at 0.6 -0.8 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "NC2"
		(at -2 1.4 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "NO2"
		(at 3.2 1.2 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(fp_text user "NC1"
		(at -2 -0.8 0)
		(unlocked yes)
		(layer "B.SilkS")
	)
	(pad "1" thru_hole oval
		(at 2.54 -3)
		(size 2 2.5)
		(drill 0.8
			(offset 0.2 0)
		)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 0 -3)
		(size 1.85 2.5)
		(drill 0.8)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at -2.54 -3)
		(size 2 2.5)
		(drill 0.8
			(offset -0.2 0)
		)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at -2.54 3)
		(size 2 2.5)
		(drill 0.8
			(offset -0.2 0)
		)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 0 3)
		(size 1.85 2.5)
		(drill 0.8)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 2.54 3)
		(size 2 2.5)
		(drill 0.8
			(offset 0.2 0)
		)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD6_USER_3DMOD_DIR}/SW_Btn_XLX.step"
		(offset (xyz 0 0 0))
		(scale (xyz 1 1 1))
		(rotate (xyz 0 0 0))
	)
)
