(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "USB_C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -26.035 13.335 0)
		)
		(property "Value" ""
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "USB_C_0_1")
		(symbol "USB_C_1_1"
			(text "USB - C\n"
				(at 0 -3.175 0)
			)
			(pin power_in line
				(at -4.445 10.795 270)
				(length 2.54)
				(name "VBUS")
				(number "1")
			)
			(pin bidirectional line
				(at -2.54 10.795 270)
				(length 2.54)
				(name "CC1")
				(number "2")
			)
			(pin bidirectional line
				(at -0.635 10.795 270)
				(length 2.54)
				(name "D-")
				(number "3")
			)
			(pin bidirectional line
				(at 1.27 10.795 270)
				(length 2.54)
				(name "D+")
				(number "4")
			)
			(pin bidirectional line
				(at 3.175 10.795 270)
				(length 2.54)
				(name "CC2")
				(number "5")
			)
			(pin power_in line
				(at 5.08 10.795 270)
				(length 2.54)
				(name "GND")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
)
