(footprint "SW_PUSH-12mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Generic SW PUSH 12mm, e.g https://sten-eswitch-13110800-production.s3.amazonaws.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
	(tags "tact sw push 12mm")
	(property "Reference" "REF**"
		(at -0.42 -7.91 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_PUSH-12mm"
		(at 0.12 8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at -6.25 -2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at -6.25 -2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole oval
		(at -6.25 -2.5)
		(size 3.2 1.9)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole oval
		(at 6.25 -2.5)
		(size 3.2 1.9)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at -6.25 2.5)
		(size 3.2 1.9)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 6.25 2.5)
		(size 3.2 1.9)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.step"
		(offset
			(xyz -6.25 2.5 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
