(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ULTRASONIC SENSOR"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" ""
			(at 0 -10.163 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "MF" ""
			(at 0 0 0)
		)
		(property "Description_1" ""
			(at 0 0 0)
		)
		(property "Package" ""
			(at 0 0 0)
		)
		(property "Price" ""
			(at 0 0 0)
		)
		(property "Check_prices" ""
			(at 0 0 0)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 0)
		)
		(property "MP" ""
			(at 0 0 0)
		)
		(property "Availability" ""
			(at 0 0 0)
		)
		(property "MANUFACTURER" ""
			(at 0 0 0)
		)
		(symbol "ULTRASONIC SENSOR_0_0"
			(pin power_in line
				(at -10.16 3.81 0)
				(length 5.08)
				(name "VCC")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 1.27 0)
				(length 5.08)
				(name "TRIG")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -1.27 0)
				(length 5.08)
				(name "ECHO")
				(number "3")
			)
			(pin power_in line
				(at -10.16 -3.81 0)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
)
