(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "BC547"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 3.81 1.905 0)
		)
		(property "Value" "BC547"
			(at 5.08 -3.302 90)
		)
		(property "Footprint" ""
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "BC547_0_1")
		(symbol "BC547_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "BASE")
				(number "2")
			)
			(pin passive line
				(at 1.27 5.08 270)
				(length 2.54)
				(name "COLLECTOR")
				(number "1")
			)
			(pin passive line
				(at 1.27 -5.08 90)
				(length 2.54)
				(name "EMITTER")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
)
