(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "rotary_encoder"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -28.448 0.762 0)
		)
		(property "Value" ""
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "rotary_encoder_0_1")
		(symbol "rotary_encoder_1_1"
			(text "ROTARY\nENCODER\n"
				(at 9.398 0 900)
			)
			(pin power_in line
				(at -3.81 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "CLK")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 1.27 7.62 270)
				(length 2.54)
				(name "DT")
				(number "2")
			)
			(pin passive line
				(at 3.81 -7.62 90)
				(length 2.54)
				(name "SWITCH")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
)
